|  |
| --- |
| **Page 1** |

ERRORMEMORY REPORT

-------------------------------------

Date: 06/20/21 12:21:20

ECU: SMG2

JobStatus: OKAY

Variant: SMG2

-------------------------------------------------- -----------

RESULT: 3 errors in error memory!

-------------------------------------------------- -----------

59 Activation of the clutch

Error frequency: 1

Error occurred 1. times at:

Mileage

202110.00 km

Ambient temperature

9.00 degrees C

Power supply Ubatt

7.17 V

Actual current of the clutch solenoid valve

1496.00 mA

Brake signals raw value

0.00 Brake not applied

Actual hydraulic temperature

12.00 degrees C

Hydraulic pressure raw value

48.27 bar

Coupling position raw value

504.00 inc

Target position clutch

377.00 inc

Motor speed from CAN

0.00 rpm

Error occurred 2. times at:

Mileage

0.00 km

Ambient temperature

-48.00 degrees C

Power supply Ubatt

0.00 V

Actual current of the clutch solenoid valve

0.00 mA

Brake signals raw value

0.00 Brake not applied

Actual hydraulic temperature

-48.00 degrees C

Hydraulic pressure raw value

-12.48 bar

Coupling position raw value

0.00 inc

Target position clutch

0.00 inc

Motor speed from CAN

0.00 rpm

Error occurred 3. times at:

Mileage

0.00 km

Ambient temperature

-48.00 degrees C

Power supply Ubatt

0.00 V

Actual current of the clutch solenoid valve

0.00 mA

Brake signals raw value

0.00 Brake not applied

Actual hydraulic temperature

-48.00 degrees C

Hydraulic pressure raw value

-12.48 bar

Coupling position raw value

0.00 inc

Target position clutch

0.00 inc

Motor speed from CAN

0.00 rpm

sporadic error

-------------------------------------------------- -----------

97 Power supply

Error frequency: 1

Error occurred 1. times at:

|  |
| --- |
| **Page 2** |

Mileage

201020.00 km

Ambient temperature

31.00 degrees C

Power supply Ubatt

9.68 V

Motor speed actual value

0.00 rpm

Not relevant

511.00 -

Not relevant

512.00 -

Not relevant

208.00 -

Not relevant

131.00 -

Not relevant

514.00 -

Not relevant

800.00 -

Error occurred 2. times at:

Mileage

0.00 km

Ambient temperature

-48.00 degrees C

Power supply Ubatt

5.38 V.

Motor speed actual value

0.00 rpm

Not relevant

512.00 -

Not relevant

513.00 -

Not relevant

208.00 -

Not relevant

507.00 -

Not relevant

809.00 -

Not relevant

522.00 -

Error occurred 3. times at:

Mileage

0.00 km

Ambient temperature

-48.00 degrees C

Power supply Ubatt

5.67 V

Motor speed actual value

0.00 rpm

Not relevant

511.00 -

Not relevant

512.00 -

Not relevant

208.00 -

Not relevant

499.00 -

Not relevant

517.00 -

Not relevant

787.00 -

implausible value

sporadic error

-------------------------------------------------- -----------

178 Level 3 security concept

Error frequency: 1

Error occurred 1. times at:

Mileage

200860.00 km

Ambient temperature

28.00 degrees C

Power supply Ubatt

11.55 V

Error code MU

5.00 -

Error code MC

0.00 -

Reset counter MC

0.00 -

Reset counter MU

1.00 -

Byte - Service brake and transmission status 17.00 -

Byte - Desired and current course i 16.00 -

Motor speed raw value in reset-proof range 1074.00 1 / min

Error occurred 2. times at:

Mileage

0.00 km

Ambient temperature

-48.00 degrees C

Power supply Ubatt

0.00 V

Error code MU

0.00 -

|  |
| --- |
| **Page 3** |

Error code MC

0.00 -

Reset counter MC

0.00 -

Reset counter MU

0.00 -

Byte - Service brake and gear status 0.00 -

Byte - Desired and current gear i 0.00 -

Motor speed raw value in the reset-proof range 0.00 1 / min

Error occurred 3. times at:

Mileage

0.00 km

Ambient temperature

-48.00 degrees C

Power supply Ubatt

0.00 V

Error code MU

0.00 -

Error code MC

0.00 -

Reset counter MC

0.00 -

Reset counter MU

0.00 -

Byte - Service brake and gear status 0.00 -

Byte - Desired and current gear i 0.00 -

Motor speed raw value in the reset-proof range 0.00 1 / min

implausible value

sporadic error

============================================================================ ===========