|  |
| --- |
| **Page 1** |

ERRORMEMORY REPORT

-------------------------------------

Date: 06/20/21 12:22:32

ECU: MSS54DS0

JobStatus: OKAY

Variant: MSS54DS0

-------------------------------------------------- -----------

RESULT: 3 errors in error memory!

-------------------------------------------------- -----------

79 Exhaust gas temperature sensor

Error frequency: 3

Logistic counter: 40

Error occurred 1. times at:

Engine speed

2000.00 rpm

relative filling

21.60%

Cooling water temp.

85.00 degrees C

Supply voltage HR

13.60 BC

occurred before (rel. BZ)

6.70 h

Error occurred 2. times at:

Engine speed

3360.00 rpm

relative filling

18.40%

Cooling water temp.

85.00 degrees C

Supply voltage HR

13.60 BC

occurred before (rel. BZ)

6.00 a.m.

Error occurred 3. times at:

Engine speed

4600.00 rpm

relative filling

10.40%

Cooling water temp.

85.00 degrees C

Supply voltage HR

13.60 BC

occurred before (rel. BZ)

0.40 h

1000 - Condition / value implausible or overtemperature

Error present at the moment

sporadic error

-------------------------------------------------- -----------

132 DSC message timeout

Error frequency: 1

Logistic counter: 32

Engine speed

0.00 rpm

relative filling

0.00%

Cooling water temp.

22.00 degrees C

Supply voltage HR

10.50 V

occurred before (rel. BZ)

6.50 h

Telegram not received

Error does not exist at the moment

sporadic error

-------------------------------------------------- -----------

68 SMG safety concept

|  |
| --- |
| **Page 2** |

Error frequency: 1

Logistic counter: 32

Engine speed

3520.00 rpm

relative filling

10.40%

Speed ​​discreet

92.00 km / h

DME status

0.00 -

occurred before (rel. BZ)

6.60 h

1000 - Condition / value implausible or overtemperature

Error does not exist at the moment

sporadic error

============================================================================ ===========